**Trafic refrigerated**

**Base vehicle :** **TRAFIC Van**

* Version : L1H1
* Engine and emission standard : M9R 2.0 dci Euro6df
* Gearbox : BVM6
* Power : 150hp, 350 N.m à 1500 rp/mn

**Conversion, coverterr : ECP**

* Internal dimensions (mm): L 2210 x l 1510 x h 1220
* Useful volume 4.2m3
* Positive cold
* PU foam and polyester sandwich panel insulation
* Possible options: Shelves, intermediate floor, fishmonger statement, wolf tooth bar, plinth
* Carrier group NEOS 100S