**Master E-Tech Benne**

**Base vehicle : Master E-Tech Electric**

* Version : Chassis Cab L3
* Moteur : Electric
* Power : 57 kW
* Battery : 52 kwh

**Conversion, converter JPM :**

GalvaZ 55 steel tipper

* 3260 x 2000 x 330 mm (internal dimensions)
* Tipping capacity: 4T3
* Bottom of container in HX500 galvanized steel sheet, th. 3mm

Rear anti-underrun bar + drawbar

* Approved towbar PTRA ≤ 7T
* Fire grids and pole lights: raised and recessed
* Mixed Crochet

PVC protectors

* Available on sides, rear door and cabin guard
* Shock absorption thanks to a flexible PVC

Load stops

* Possibility of wedging and strapping a load on the cabin guard